◄Previous: 4.3 Digital Subscriber Line (DSL) broadband

# 4.4 VDSL2

VDSL2 (version 2 of Very High Bit Rate DSL) achieves higher data rates than ADSL by shortening the copper line. Shortening results from the use of a locally installed connection box like Figure 25.

Figure 25 Fibre box used with VDSL2

The box contains, effectively, a piece of telephone-exchange equipment which is linked to the local exchange by optical fibre. Subscribers have the copper line from their home terminated at the box – at least as far as data is concerned. (Telephony continues to use copper wire to the exchange.)

Because signal attenuation per metre of copper wire increases with increasing frequency, a major benefit of a short copper line is that higher frequencies can be used and therefore more subchannels made available. VDSL2 uses many more subchannels than any version of ADSL. Various frequency plans, or profiles, are available for VDSL2. Figure 26 is a common one, called ‘17a’, in which the highest frequency is just above 17 MHz.

Figure 26 VDSL2 profile 17a

Downstream data rates with VDSL2 are typically around 30 to 80 Mbit s–1, and upstream rates can be in the region of 20 Mbit s–1, although providers often set a lower rate.

Figure 27 is a setting screen from a domestic VDSL2 broadband router. A range of VDSL2 profiles is shown; and because the symbol rate and subchannel width are standard across VDSL2 and ADSL the router can also cope with ADSL (as evident in the ‘Modulation’ row). ‘G.DMT’ is an informal name for the first ADSL standard, now usually referred to as ADSL1. ‘G.lite’ is a very basic form of ADSL that did not catch on. ‘SRA’ is Seamless Rate Adaptation and is one way of dynamically changing the speed of the connection according to noise conditions.

Figure 27 Settings screen of a domestic DSL router
◄Contents►Next: 4.5 4G mobile broadband

OpenLearn - Exploring communications technology
Except for third party materials and otherwise, this content is made available under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 Licence, full copyright detail can be found in the acknowledgements section. Please see full copyright statement for details.