# 4.7 Mars Reconnaissance Orbiter

In 2005, NASA sent its most powerful orbiter (even to date, 2021) to Mars. The Mars Reconnaissance Orbiter (MRO) is equipped with a number of instruments with which to image the surface, determine its mineralogy and even investigate the subsurface.

Figure 37 shows a stunning example of an image taken by MRO’s High Resolution Imaging Science Experiment (HiRISE), capable of imaging the surface of Mars at 30 cm per pixel. It shows horizontal layers or beds that are probably sedimentary rocks deposited in a standing body of water. These beds also appear to be disrupted, possibly by episodic flooding. Sedimentary beds can also be seen on Figure 38, which shows the floor of the Ebersawalde impact crater, further evidence of significant bodies of liquid water in Mars’ past.

Figure 37 HiRISE image taken of Ladon Vallis, a 600 km-long outflow channel extending from a basin in the south to the north of Mars. The light-toned layers contrast with the darker-toned deposit on the floor of the channel, with dark toned dunes partly filling fractures and impact craters. Credit: NASA/JPL-Caltech/University of Arizona.
Figure 38 HiRISE image of the floor of an impact crater north of Ebersawalde crater. Credit: NASA/JPL-Caltech/University of Arizona.

HiRISE has also identified processes that are happening now on Mars. Figure 39 shows two images taken three years apart. Comparing these, you can see a new channel (labelled with an arrow) on the more recent, right-hand image that is absent in the older image. This means a process is operating now on the martian surface that can produce features such as this. Although at first this was thought to be a process involving water, it is now believed to be formed by the sublimation of carbon dioxide frost over the martian winter. Similar processes are thought to be responsible for other surface features (e.g., Figure 40), but this shows that geomorphology is not always a reliable tool with which to look for water.

Figure 39 Pair of HiRISE images taken in 2010 (left) and 2013 (right), showing a new channel, as indicated by the white arrow, formed by seasonal variation in carbon dioxide frost. Other HiRISE observations have indicated that these processes typically occur gradually in winter. Credit: NASA/JPL-Caltech/Univ. of Arizona.

This browser does not support video playback.

Figure 40 Animation of a series of images acquired by HiRISE between 2007 and 2013. The animation shows the transition of carbon dioxide from ice to gas (sublimation) at the south pole of Mars. As the ice sublimates from the walls of the pit it reforms on nearby flat surfaces. Credit: NASA/JPL-Caltech/University of Arizona.

MRO has two other instruments important to the search for water. The CRISM (Compact Reconnaissance Imaging Spectrometer for Mars) instrument can detect minerals on the martian surface at a resolution of 18 m per pixel. Consistent with previous spacecraft, it has found widespread clay minerals, but has also identified sulfates and carbonates. These were previously unseen by lower resolution orbiting instruments but had been identified by spacecraft on the martian surface. Figure 41 shows a false-colour image created using CRISM data to highlight the distribution of certain minerals in Jezero crater. These data were key in selecting this crater as the landing site for the NASA Perseverance rover, which you will hear more about later.

Figure 41 Topographic image with CRISM false-colour imagery overlain. Green suggests carbonate minerals (formed by water) and red indicates olivine sand. Credit: NASA/JPL-Caltech/MSSS/JHU-APl/Purdue/USGS.

MRO also carries SHARAD (SHAllow RADar sounder), a radar instrument, like MARSIS on Mars Express. This has found that the ice at the north pole is around 2 km thick and has internal layers (Figure 42), but it has also found ice at other areas of Mars, located approximately 90 m below the surface (Figure 43).

Figure 42 SHARAD radar cross section of the north polar cap of Mars You can see an internal ice structure with the white lines representing radar reflections due to layers/boundaries. Credit: NASA/JPL-Caltech/ASI/UT.
Figure 43 SHARAD radargram showing subsurface water ice in Utopia Planitia region of Mars. The white arrows indicate subsurface reflections caused by the subsurface water ice. Credit: NASA/JPL-Caltech/Univ. of Rome/ASI/PSI.

OpenLearn - The search for water on Mars
Except for third party materials and otherwise, this content is made available under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 Licence, full copyright detail can be found in the acknowledgements section. Please see full copyright statement for details.