Manufacturing

## 2.2 Properties for processing – casting

### 2.3 Types of casting

◄Previous: 2.2 Properties for processing – casting

# 2.3.1 Permanent pattern

This type of casting uses a model, or pattern, of the final product to make an impression which forms the mould cavity. Each mould is destroyed after use but the same pattern is used over and over again. Sand casting is a typical example of a permanent pattern process, where a pattern is placed into a special casting sand to form the right shape of cavity. Permanent pattern processes are usually cheaper than other methods, especially for small quantity production or 'one-offs', and are suitable for a wide range of sizes of product.

◄Contents►Next: 2.3.2 Permanent mould

OpenLearn - Manufacturing
Except for third party materials and otherwise, this content is made available under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 Licence, full copyright detail can be found in the acknowledgements section. Please see full copyright statement for details.