Manufacturing

# 2.3.2 Permanent mould

In this method the same mould is used for large numbers of castings. Each casting is released by opening the mould rather than by destroying it. Permanent moulds need to be made of a material which can withstand the temperature fluctuations and wear associated with repeated casting. A good example of a product made with methods such of this is the ubiquitous 'die-cast' child's toy ('die' is another word for 'mould').

Figure 18 Die-cast toy
Figure 18
View long description

OpenLearn - Manufacturing
Except for third party materials and otherwise, this content is made available under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 Licence, full copyright detail can be found in the acknowledgements section. Please see full copyright statement for details.