Engineering: The challenge of temperature

## 4.4 Summary of Section 4

### 5 Sudden temperature effects

# 5.1 Sudden changes

The third category of thermal effects identified in Section 2 are those associated with sudden changes. Here are some technically important examples where things change suddenly at a particular temperature:

- Pure water boils at 100 °C (at atmospheric pressure).

- An alloy of neodymium, iron and boron (sometimes written NdFeB, although this is not a quantitative chemical formula) that is widely used for permanent magnets in small, compact motors will lose its magnetisation when heated beyond 450 °C.

- Pure gold melts at 1063 °C (at atmospheric pressure).

- Silver and oxygen spontaneously combine to form silver oxide if the temperature is less than 1530 °C, although the rate of oxidation is extremely slow at ambient temperature. Above 1530 °C the reverse process is spontaneous and silver oxide decomposes into its component parts.

- The compound yttrium-barium-copper oxide (YBCO, pronounced 'ibco') loses all its electrical resistivity below about −180 °C (i.e. it becomes a superconductor).

In each of these examples matter is undergoing a change of phase. Establishing a little more precisely what that means is the goal of Section 5.2. After that, we'll see if there is any scope here for devising thermal cut-outs.

OpenLearn - Engineering: The challenge of temperature
Except for third party materials and otherwise, this content is made available under a Creative Commons Attribution-NonCommercial-ShareAlike 4.0 Licence, full copyright detail can be found in the acknowledgements section. Please see full copyright statement for details.